For 1990-2009 cars

Callout | Component Name
--- | ---

#### Headlamp Washer Solvent Container Replacement

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.
3. Remove the air deflector assembly. Refer to Front Air Deflector Replacement.

1 | Hood Front Compartment Housing Retainer (qty: 6)
2 | Hood Front Compartment Assembly
3 | Front Bumper Fascia Extension Retainer (qty: 11)
4 | Front Bumper Fascia Extension Tip Right Hand only
5 | Front Bumper Fascia Extension Trim Assembly Refer to Fascia, Extension, Reinforcement and Impact Bar Replacement - Front Bumper.
6 | Headlamp Assembly Refer to Headlamps, Fog Lamps, Turn Signal Lamps, Side Marker Lamps Replacement - Front . Tip Right Hand only
7 | Washer Container Cap
8 | Windshield Washer Solvent Container Screws (qty:3) Notice: Refer to Fastener Notice in the Preface section. Tighten 9 N·m (80 lb in)
9 | Windshield Washer Fluid Reservoir Assembly