For 1990-2009 cars

Checks | Causes
--- | ---
Center (with 2-6 Low and Reverse Clutch) Support Assembly (67) |

• | Inspect for damaged or worn 2-6 clutch plates (452 and 454).

• | Inspect for damaged 2-6 clutch backing plate (451). Inspect for worn splines on backing plate.

• | Inspect for damaged 2-6 clutch backing plate retaining ring (450).

• | Inspect for damaged 2-6 clutch piston assembly (457), spring (456), retaining ring (455), and center support assembly (459).