For 1990-2009 cars

### Left Side Harness Connections

1. Connect the engine wiring harness to the left side fuel injectors.
2. Connect the engine wiring harness to the left camshaft cover.
3. Connect the engine wiring harness to the left coil assembly harness.
4. Connect the engine wiring harness to the left camshaft position sensors.
5. Connect the engine wiring harness to the evaporative emission (EVAP) purge solenoid.
6. Connect the engine wiring harness to the throttle position sensor on the throttle body.
7. Connect the engine wiring harness to the air conditioner compressor.
8. Connect the engine wiring harness to the oil pressure sensor.

### Right Side Harness Connections

1. Connect the engine wiring harness to the right side fuel injectors.
2. Connect the engine wiring harness to the right camshaft cover.
3. Connect the engine wiring harness to the right coil assembly harness.
4. Connect the engine wiring harness to the right camshaft position sensors.
5. Connect the engine wiring harness ground to the intake manifold stud.

Caution: Refer to Fastener Caution in the Preface section.

6. Install the engine wiring harness ground nut.

Tighten
Tighten the engine wiring harness ground nut to 10 N·m (89 lb in).

7. Connect the engine wiring harness to the ECT sensor at the rear of the right cylinder head.
8. Connect the engine wiring harness to the generator.
9. Connect the starter motor wiring harness to the generator.
10. Install the starter motor wiring harness generator nut.

Tighten
Tighten the starter motor wiring harness generator nut to 10 N·m (89 lb in).

11. Connect the engine wiring harness to the MAP sensor.
12. Connect the engine wiring harness to the knock and crankshaft position sensor wiring harness.
13. Install the engine wiring harness bracket to the side of the right cylinder head.
14. Install the engine wiring harness bracket bolts.

Tighten
Tighten the engine wiring harness bracket bolts to 45 N·m (33 lb ft).