For 1990-2009 cars

### Removal Procedure

1. Remove the left closeout/insulator panel. Refer to Instrument Panel Insulator Replacement - Left Side
2. Remove the torque converter clutch/cruise release switch (3) by pulling the upper switch out of the retainer.
3. Disconnect the electrical connector from the torque converter clutch/cruise release switch (3).

### Installation Procedure

1. Connect the electrical connector to the torque converter clutch/cruise release switch (3).
2. Install the torque converter clutch/cruise release switch (3) into the upper retainer.
3. Adjust the torque converter clutch/cruise release switch. Refer to Torque Converter Clutch/Cruise Control Release Switch Adjustment .
4. Install the left closeout/insulator panel. Refer to Instrument Panel Insulator Replacement - Left Side