For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the rear compartment lid inner panel trim assembly. Refer to Rear Compartment Lid Inner Panel Trim Replacement.
2. Remove the rear compartment inner panel access plugs to gain access to the outboard spoiler nuts.

1 | Rear End Spoiler Nut (Qty: 8) Caution: Refer to Fastener Caution in the Preface section. Tighten 6 N·m (53 lb in)
2 | Rear End Spoiler Assembly