For 1990-2009 cars

Callout | Component Name
--- | ---

#### Front Side Door Assembly Replacement

1 | Front Side Door Check Link Bolt Notice: Refer to Fastener Notice in the Preface section. Tighten 9 N·m (80 lb in)
2 | Front Door Wiring Harness Tip Disconnect door wiring harness and reconnect when replacement is complete.
3 | Front Side Door Hinge Lower Bolt (Qty: 2) Tighten 25 N·m (18 lb ft)
4 | Front Side Door Hinge Upper Bolt (Qty: 2) Tighten 25 N·m (18 lb ft)
5 | Front Side Door Assembly Notice: Striker alignment is a crucial part of door latch operation. Do not use the door striker to adjust the door to the vehicle. Failure to properly adjust the striker can result in damage to the door latch and the striker.

Tip
Check the door for proper alignment, adjust as necessary. Refer to Door Adjustment .

#### Front Side Door Lower Hinge Assembly Replacement

Tip
Replace only one hinge at a time.

3 | Front Side Door Hinge Lower Bolt (Qty: 2) Tighten 25 N·m (18 lb ft)
6 | Front Side Door Hinge Lower Bolt (Qty: 2) Tighten 25 N·m (18 lb ft)
7 | Front Side Door Lower Hinge Assembly Notice: Striker alignment is a crucial part of door latch operation. Do not use the door striker to adjust the door to the vehicle. Failure to properly adjust the striker can result in damage to the door latch and the striker.

Tip
Check the door for proper alignment, adjust as necessary. Refer to Door Adjustment .

#### Front Side Door Upper Hinge Assembly Replacement

Tip
Replace only one hinge at a time.

4 | Front Side Door Hinge Upper Bolt (Qty: 2) Tighten 25 N·m (18 lb ft)
8 | Front Side Door Hinge Upper Bolt (Qty: 2) Tighten 25 N·m (18 lb ft)
9 | Front Side Door Upper Hinge Assembly Notice: Striker alignment is a crucial part of door latch operation. Do not use the door striker to adjust the door to the vehicle. Failure to properly adjust the striker can result in damage to the door latch and the striker.

Tip
Check the door for proper alignment, adjust as necessary. Refer to Door Adjustment .