For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Bolt M6 x 20 (Qty: 18)
2 | Fluid Pan Assembly
3 | Fluid Pan Gasket Tip The fluid pan gasket is reusable. Inspect the gasket to determine if it may be reused. If the gasket is stuck to the case or pan, it should be replaced.
4 | Fluid Filter Assembly Notice: Pull the fluid filter assembly straight out to avoid damage. Do not bend or twist the filter neck.
5 | Fluid Filter Seal Assembly Notice: Do not damage the case sealing surface when removing the filter seal assembly. Tip Use a screwdriver or snap ring pliers.
6 | Electrical Connector Slide Lock Notice: Pull up on the electrical connector slide lock to avoid damage to the connector.
7 | Electrical Connector Passage Sleeve

#### Special Tools

• | DT 47715 Electrical Connector Passage Sleeve Remover/Installer

• | J 42183 Driver Handle