For 1990-2009 cars

### Removal Procedure

1. Turn the ignition OFF.
2. Remove the front compartment sight shields if necessary. Refer to Sight Front Compartment Sight Shields Replacement .
3. Remove the positive crankcase ventilation (PCV) hose from the air cleaner duct resonator.
4. Loosen the air cleaner duct clamps.
5. Remove the air cleaner duct.

### Installation Procedure

1. Install the air cleaner intake duct.
2. Install the PCV hose to the intake duct resonator.

Notice: Refer to Fastener Notice in the Preface section.

3. Tighten the air cleaner duct clamps.

Tighten
Tighten the clips to 4 N·m (35 lb in).

4. Install the front compartment sight shields as necessary. Refer to Front Compartment Sight Shields Replacement .