For 1990-2009 cars

### Removal Procedure

1. Remove the bridge console. Refer to Front Floor Console Extension Replacement - Center .
2. Remove the front floor console extension trim panel. Refer to Front Floor Console Extension Panel Replacement .
3. Remove the console shift lever bezel. Refer to Console Shift Lever Bezel Replacement .
4. Remove the ashtray assembly. Refer to Ashtray Side Panel Replacement .
5. Remove the bolts securing the front floor console to the I/P carrier.
6. Remove the bolts securing the rear of the front floor console to the floor.
7. Disconnect the electrical connector, and remove the front floor console rearward and upward.

### Installation Procedure

1. Connect the electrical connector, and install the front floor console.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolts securing the rear of front floor console to the floor.

Tighten
Tighten the bolts to 9 N·m (80 lb in).

3. Install the bolts securing the front floor console to the I/P carrier.

Tighten
Tighten the bolts to 9 N·m (80 lb in).

4. Install the ashtray assembly. Refer to Ashtray Side Panel Replacement .
5. Install the console shift lever bezel. Refer to Console Shift Lever Bezel Replacement .
6. Install the front floor console extension trim panel. Refer to Front Floor Console Extension Panel Replacement .
7. Install the bridge console. Refer to Front Floor Console Extension Replacement - Center .