For 1990-2009 cars

### Circuit Description

The HVAC control module monitors the evaporator temperature via the evaporator temperature sensor. When the air is cold, the sensor resistance and signal voltage are high. When the air is warm, the sensor resistance and signal voltage are low.

### DTC Descriptor

The diagnostic procedure supports the following DTCs:

• | DTC B3933 Evaporator Temperature Sensor Circuit

• | DTC P1531 Air Conditioning (A/C) Evaporator Temperature Sensor Circuit

This vehicle has DTCs which include DTC Symptoms. For more information on DTC Symptoms, refer to DTC Symptom Description .

DTC Symptom | DTC Symptom Descriptor
--- | ---
00 | Out of Range Condition

### Conditions for Running the DTC

The ignition is ON.

### Conditions for Setting the DTC

The HVAC control module detects the evaporator temperature sensor signal circuit is less than 0.09 volt (5 counts) or greater than 4.90 volts (250 counts).

### Action Taken When the DTC Sets

• | The driver information center (DIC) will display SERVICE A/C SYSTEM.

• | The A/C OFF segment will illuminate on the HVAC control module.

• | The A/C compressor will be disabled.

### Conditions for Clearing the DTC

• | The DTC will become history if the HVAC control module no longer detects a failure.

• | The history DTC will clear after 50 fault-free ignition cycles.

• | The DTC can be cleared with a scan tool.

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. This step tests for the proper operation of the circuit in the high voltage range.

2. This step tests for the proper operation of the circuit in the low voltage range. If the fuse in the jumper opens upon performing this test, the signal circuit has a short to voltage.

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
Schematic Reference: HVAC Schematics Connector End View Reference: HVAC Connector End Views
1 | Did you perform the Diagnostic System Check - Vehicle? | -- | Go to Step 2 | Go to Diagnostic System Check - Vehicle
2 |

1. Install a scan tool.
2. Turn ON the ignition, with the engine OFF.
3. With a scan tool, observe the Evaporator Temp parameter in the Climate Control Panel, Open/Short data list.

Does the scan tool indicate that the Evaporator temp parameter is within the specified range?

0.09-4.90 V

Go to Testing for Intermittent Conditions and Poor Connections

Go to Step 3

3 |

1. Turn OFF the ignition.
2. Disconnect the evaporator temperature sensor.
3. Turn ON the ignition, with the engine OFF.
4. With a scan tool, observe the Evaporator Temp parameter.

Is the Evaporator Temp parameter greater than the specified value?

4.90 V

Go to Step 4

Go to Step 5

4 |

1. Turn OFF the ignition.
2. Connect a 3-amp fused jumper wire between the signal circuit of the evaporator temperature sensor and the low reference circuit of the evaporator temperature sensor.
3. Turn ON the ignition, with the engine OFF.
4. With a scan tool, observe the Evaporator Temp parameter.

Is the Evaporator Temp parameter less than the specified value?

0.09 V

Go to Step 9

Go to Step 6

5 | Test the signal circuit of the evaporator temperature sensor for a short to ground. Refer to Circuit Testing and Wiring Repairs . Did you find and correct the condition? | -- | Go to Step 13 | Go to Step 10
6 | Test the signal circuit of the evaporator temperature sensor for one of the following conditions:

• | A short to voltage

• | A high resistance

• | An open circuit

Refer to Circuit Testing and Wiring Repairs .

Did you find and correct the condition?

--

Go to Step 13

Go to Step 7

7 | Test the low reference circuit of the evaporator temperature sensor for one of the following conditions:

• | A high resistance

• | An open circuit

Refer to Circuit Testing and Wiring Repairs .

Did you find and correct the condition?

--

Go to Step 13

Go to Step 8

8 | Test the following signal circuits for a short to voltage:

• | Inside air temperature sensor

• | Ambient air temperature sensor

• | Left sunload sensor

• | Right sunload sensor

• | Ambient light sensor

Refer to Circuit Testing and Wiring Repairs .

Did you find and correct the condition?

--

Go to Step 13

Go to Step 10

9 | Inspect for poor connections at the harness connector of the evaporator temperature sensor. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs . Did you find and correct the condition? | -- | Go to Step 13 | Go to Step 11
10 | Inspect for poor connections at the harness connector of the HVAC control module. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs . Did you find and correct the condition? | -- | Go to Step 13 | Go to Step 12
11 | Replace the evaporator temperature sensor. Refer to Auxiliary Temperature Valve Actuator Replacement . Have you finished the replacement? | -- | Go to Step 13 | --
12 | Replace the HVAC control module. Refer to HVAC Control Module Replacement for replacement, setup, and programming. Have you finished the replacement? | -- | Go to Step 13 | --
13 |

1. Use the scan tool in order to clear the DTCs.
2. Operate the vehicle within the Conditions for Running the DTC.

Does the DTC reset?

--

Go to Step 2

System OK