For 1990-2009 cars

1. 1. Inspect the bearing rollers and races for the following conditions:

• | Pitting

• | Scoring or grooves

• | Excessive wear or other damage

2. Inspect the bearing rollers and races for heat discoloration.

Heat discoloration ranges from a faint yellow to a dark blue color. This discoloration may result from an overload or improper lubrication. Excessive heat causes softening of the rollers and races. Bearings or races with sign of heat discoloration must be replaced.

3. Inspect bearing holder for bent.
4. Inspect for bearing holder for damage.