For 1990-2009 cars

1. Loosen the fasteners (2) that secure the hood to the hood hinges (1).
2. Adjust the hood in order to obtain an even gap on both sides between the hood and the fenders and so that the hood is flush with both fenders on the front edge.

Caution: Refer to Fastener Caution in the Preface section.

3. Tighten the fasteners (2) that secure the hood to the hood hinges (1).

Tighten
Tighten the fasteners to 9 N·m (80 lb in).