For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front seats. Refer to Driver or Passenger Seat Replacement.
2. Remove the front seat cushion retaining nuts. Refer to Driver or Passenger Seat Back Ventilation Heating and Cooling Blower Replacement.
3. Re-zero the inflatable restraint passenger presence system whenever the seat cushion or any component of the passenger presence system is removed. Refer to Passenger Presence System Programming and Setup .

1 | Seat Cushion Frame Refer to Driver or Passenger Seat Back Ventilation Heating and Cooling Blower Replacement.
2 | Front Seat Control Module Retaining Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 2N·m (18 lb in)
3 | Front Seat Control Module Tip Reprogram memory seat module when replacing the seat control module.