For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery Cable to Battery Bolt | 17 N·m | 13 lb ft
Battery Negative Cable to Engine Block Bolt (LH2) | 25 N·m | 18 lb ft
Battery Negative Cable to Engine Block Stud (LY7) | 50 N·m | 37 lb ft
Battery Negative Cable to Shock Tower Bolt (LH2) | 10 N·m | 89 lb in
Battery Positive Cable to Side Rail Bolt (LY7) | 36 N·m | 27 lb ft
Battery Positive Cable to Starter Terminal Nut (LH2) | 10 N·m | 89 lb in
Battery Positive Cable to Starter Terminal Nut (LY7) | 13 N·m | 115 lb in
Battery Positive Cable to Underhood Fuse Block Nut | 15 N·m | 11 lb ft
Battery Retainer Bolt | 18 N·m | 13 lb ft
Battery Tray Bolt | 6 N·m | 53 lb in
Generator Bracket Bolt | 50 N·m | 37 lb ft
Generator Bracket Bolt (LY7) | 23 N·m | 17 lb ft
Generator Bolt (LH2) | 50 N·m | 37 lb ft
Generator Bolt (LY7) | 46 N·m | 34 lb ft
Generator Output Battery Terminal Nut (LH2) | 10 N·m | 89 lb in
Generator Output Battery Terminal Nut (LY7) | 13 N·m | 115 lb in
Ground Strap to Cam Cover Bolt (LH2) | 10 N·m | 89 lb in
Ground Strap to Cylinder Head Bolt (LH2) | 25 N·m | 18 lb ft
Starter Motor Bolt (LH2) | 30 N·m | 22 lb ft
Starter Motor Bolt (LY7) | 50 N·m | 37 lb ft
Starter Motor Bolt | 51 N·m | 38 lb ft
Starter Solenoid S Terminal Nut (LH2) | 4 N·m | 35 lb in