For 1990-2009 cars

#### Special Tools

J 22912-B Rear Pinion and Axle Bearing Remover

Important: Differential gear has a requirement of preload and cannot be disassembled or assembled at random.

1. Remove the 10 ring gear bolts (1) and the ring gear (3) from the differential carrier (2) using a punch and a hammer through the bolt hole.
2. Using J 22912-B and a press, remove the left side bearing. It may be necessary to cut the bearing holder and remove the rollers so that the tool will grip the bearing race.
3. Using J 22912-B and a press, remove the right side bearing. It may be necessary to cut the bearing holder and remove the rollers so that the tool will grip the bearing race.