For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C

- Compressor Bolt - Front

23 N·m

17 lb ft

- Compressor Bracket Bolt - Rear

50 N·m

37 lb ft

- Compressor Hose Assembly Bolt

9 N·m

80 lb in

Camshaft Cap Bolt | 10 N·m | 89 lb in
Camshaft Cover Bolt | 10 N·m | 89 lb in
Camshaft Intermediate Drive Sprocket Bolt - Idler Sprocket | 58 N·m | 43 lb ft
Camshaft Position Actuator

- Camshaft Bolt

58 N·m

43 lb ft

- Oil Control Valve Bolt

10 N·m

89 lb in

Camshaft Position Sensor Bolt | 10 N·m | 89 lb in
Catalytic Converter Exhaust Manifold Nut

- Exhaust Manifold Nut

50 N·m

37 lb ft

Close Out Cover Bolt | 10 N·m | 89 lb in
Connecting Rod Bolt

- First Pass

30 N·m

22 lb ft

- Second Pass - Counterclockwise

Back Off to Zero

- Third Pass

25 N·m

18 lb ft

- Final Pass

110 Degrees

Coolant Outlet Bolt | 10 N·m | 89 lb in
Crankshaft Balancer Bolt

- First Pass

100 N·m

74 lb ft

- Final Pass

150 Degrees

Crankshaft Main Bearing Bolt
Inner

- First Pass

20 N·m

15 lb ft

- Final Pass

80 Degrees

Outer

- First Pass

15 N·m

10 lb ft

- Final Pass

110 Degrees

Side

- First Pass

30 N·m

22 lb ft

- Final Pass

60 Degrees

Crankshaft Position Sensor Bolt | 10 N·m | 89 lb in
Crankshaft Rear Oil Seal Housing Bolt | 10 N·m | 89 lb in
Cylinder Head Bolt - M8

- First Pass

15 N·m

10 lb ft

- Final Pass

60 Degrees

Cylinder Head Bolt - M11

- First Pass

45 N·m

33 lb ft

- Final Pass

120 degrees

Cylinder Head Core Hole Plug | 31 N·m | 23 lb ft
Drive Belt

- Idler Pulley Bolt

50 N·m

37 lb ft

- Tensioner Bolt

50 N·m

37 lb ft

ECM

- Bolt

10 N·m

89 lb in

- Bracket Bolt - Front

23 N·m

17 lb ft

- Bracket Bolt - Side

10 N·m

89 lb in

- Grounding Bolt

4.5 N·m

40 lb in

ECT Sensor | 22 N·m | 16 lb ft
Engine Flywheel Bolt

- First Pass

30 N·m

22 lb ft

- Final Pass

45 Degrees

Engine Front Cover Bolt | 23 N·m | 17 lb ft
Engine Mount

- Bracket Bolt

60 N·m

44 lb ft

- Nut

80 N·m

59 lb ft

Engine Wiring Harness Bracket

- Bolt - Cylinder Head Rear

40 N·m

30 lb ft

- Bolt - ECM Bracket Side

23 N·m

17 lb ft

- Bolt - ECM Bracket Top

10 N·m

89 lb in

- Bolt - Left Side Oil Filter Adapter

10 N·m

89 lb in

- Bolt - Left Side Oil Pan

10 N·m

89 lb in

- Bolt - Near Crankshaft Position Sensor

50 N·m

37 lb ft

- Bolt - Right Side Block Front

23 N·m

17 lb ft

- Bolt - Right Side Head Front

10 N·m

89 lb in

Engine Wiring Harness Ground

- Bolt - ECM Bracket Top

10 N·m

89 lb in

- Bolt - Left Cylinder Head Side

10 N·m

89 lb in

- Bolt - Right Cylinder Head Rear

10 N·m

89 lb in

EVAP Purge Valve Bolt | 10 N·m | 89 lb in
Exhaust Manifold

- Bolt

20 N·m

15 lb ft

- Heat Shield Bolt

10 N·m

89 lb in

Fuel Rail Bolt | 10 N·m | 89 lb in
Generator

- Bolt

50 N·m

37 lb ft

- Bracket Bolt - Front

50 N·m

37 lb ft

- Bracket Bolt - Side

22 N·m

16 lb ft

- Cable Nut

13 N·m

115 lb in

Ground Cable Bolt | 50 N·m | 37 lb ft
Heater Inlet/Outlet Pipe Assembly Bolt | 10 N·m | 89 lb in
Ignition Coil Bolt | 10 N·m | 89 lb in
Intake Manifold

- Brace Bolt - Engine Front Cover M12

65 N·m

48 lb ft

- Brace Bolt/Ball Stud - Intake Manifold M6

10 N·m

89 lb in

- Sight Shield Ball Stud

9 N·m

80 lb in

- Tuning Valve Bolt

10 N·m

89 lb in

- Upper-to-Cylinder Head Bolt - Long

23 N·m

17 lb ft

- Upper-to-Cylinder Head Bolt - Short

23 N·m

17 lb ft

- Upper-to-Lower Intake Manifold Bolt

23 N·m

17 lb ft

Knock Sensor Bolt | 23 N·m | 17 lb ft
MAP Sensor Bolt | 10 N·m | 89 lb in
Oil Drain Plug | 25 N·m | 18 lb ft
Oil Filter Cap | 25 N·m | 18 lb ft
Oil Filter Housing Adapter

- Bolt - Cylinder Head M10

65 N·m

48 lb ft

- Bolt - Engine Block M8

23 N·m

17 lb ft

Oil Gallery Plug - M20 | 75 N·m | 55 lb ft
Oil Galleryy Plug - M14 | 50 N·m | 27 lb ft
Oil Level Indicator Tube Bolt | 10 N·m | 89 lb in
Oil Pan

- Bolt - Block M8

23 N·m

17 lb ft

- Bolt - Crankshaft Rear Oil Seal Housing M6

10 N·m

89 lb in

- Windage Tray Bolt

10 N·m

89 lb in

Oil Pressure Sender | 20 N·m | 15 lb ft
Oil Pump

- Bolt

23 N·m

17 lb ft

- Cover Bolt

13 N·m

115 lb in

Oxygen Sensor

- Pump Converter Pipe

40 N·m

30 lb ft

PCV Tube Bracket Bolt | 10 N·m | 89 lb in
Piston Oil Cooling Nozzle Bolt | 10 N·m | 89 lb in
Power Steering Pump

- Bracket to Engine Bolt

50 N·m

37 lb ft

- Pump to Bracket Bolt

22 N·m

16 lb ft

- Reservoir Bolt - Lower

40 N·m

30 lb ft

- Reservoir Bolt - Upper

10 N·m

89 lb in

Primary Camshaft Drive Chain

- Left Lower Guide Bolt - Oil Pump - Second Design

23 N·m

17 lb ft

- Tensioner Bolt

23 N·m

17 lb ft

- Upper Guide Bolt

23 N·m

17 lb ft

Radiator Outlet Pipe

- Bolt - Generator Bracket

10 N·m

89 lb in

- Bolt - Right Cylinder Head Rear

50 N·m

37 lb ft

- Bolt - Thermostat Housing

10 N·m

89 lb in

Secondary Camshaft Drive Chain

- Guide Bolt

23 N·m

17 lb ft

- Shoe Bolt

23 N·m

17 lb ft

- Tensioner Bolt

23 N·m

17 lb ft

Spark Plug | 18 N·m | 13 lb ft
Starter Motor

- Bolt

50 N·m

37 lb ft

- Cable Nut

13 N·m

115 lb in

Suction Screen Bolt | 10 N·m | 89 lb in
Suction Tube Bolt | 10 N·m | 89 lb in
Thermostat Housing Bolt | 10 N·m | 89 lb in
Throttle Body Bolt | 10 N·m | 89 lb in
Torque Converter Bolt | 60 N·m | 44 lb ft
Transmission

- Mount Bolt

60 N·m

44 lb ft

- Range Selector Lever Nut

9.5 N·m

84 lb in

- To Engine Bolt

50 N·m

37 lb ft

Water Pump

- Bolt

10 N·m

89 lb in

- Pulley Bolt

10 N·m

89 lb in