For 1990-2009 cars

Callout | Component Name
--- | ---

#### Radiator Grille Assembly Replacement

#### Preliminary Procedures

1. Remove the front hood. Refer to Hood Replacement .
2. Remove the retainer holding the fascia to the tie bar (Qty: 4), pull the front fascia top outward so as to access the fascia grille retainer.

1 | Radiator Grille Retainer (Qty: 4) Tip There are 2 retainers at each end of the grille.
2 | Radiator Grille Assembly
3 | Radiator Grille Insert