For 1990-2009 cars

### Removal Procedure

1. Remove the rear compartment trim panel. Refer to Rear Compartment Sill Trim Plate Replacement.
2. Remove the bolts securing the amplifier to the vehicle.
3. Disconnect the electrical connector.
4. Remove the amplifier.

### Installation Procedure

1. Connect the electrical connectors.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the bolts securing the amplifier to the vehicle.

Tighten
Tighten the bolts (1) to 9 N·m (80 lb in).

3. Install the rear compartment trim. Refer to Rear Compartment Sill Trim Plate Replacement.