For 1990-2009 cars

### Removal Procedure

Warning: Refer to SIR Warning in the Preface section.

1. Disable the SIR system. Refer to SIR Disabling and Enabling.
2. Remove the inflatable restraint steering wheel module. Refer to Steering Wheel Inflatable Restraint Module Replacement.
3. Remove the retaining screws from the steering wheel control switch.
4. Disconnect the electrical connector. Remove the steering wheel control switch.

### Installation Procedure

1. Connect the electrical connector.
2. Install the steering wheel control switch retaining screw.
3. Install the inflatable restraint steering wheel module. Refer to Steering Wheel Inflatable Restraint Module Replacement
4. Enable the SIR system. Refer to SIR Disabling and Enabling.