For 1990-2009 cars

### Removal Procedure

Caution: Refer to SIR Caution in the Preface section.

1. Disable the SIR system. Refer to SIR Disabling and Enabling Zone 3 .
2. Remove the steering column from the vehicle. Refer to Steering Column Replacement.
3. Remove the following from the steering shaft:

3.1. | The boot seal (5)

3.2. | The steering shaft seal (4)

3.3. | The sensor retainer (3)

3.4. | The sensor locator (2)

4. Remove the steering wheel position sensor (1). Refer to Steering Wheel Position Sensor Centering.
5. Remove the adapter and bearing assembly from the steering column support assembly.

### Installation Procedure

1. Install the adapter and bearing assembly onto the steering column support assembly.
2. Install the following to the steering shaft:

2.1. | The steering wheel position sensor (1)--Refer to Steering Wheel Position Sensor Centering.

2.2. | The sensor locator (2)

2.3. | The sensor retainer (3)

2.4. | The steering shaft seal (4)

2.5. | The boot seal (5)

3. Install the steering column to the vehicle. Refer to Steering Column Replacement.
4. Enable the SIR system. Refer to SIR Disabling and Enabling Zone 3 .