For 1990-2009 cars

Icon | Icon Definition
--- | ---
| Important: Twisted-pair wires provide an effective shield that helps protect sensitive electronic components from electrical interference. Important: In order to prevent electrical interference from degrading the performance of the connected components, you must maintain the proper specification when making any repairs to the twisted-pair wires shown :

• | The wires must be twisted a minimum of 9 turns per 31 cm (12 in) as measured anywhere along the length of the wires.

• | The outside diameter of the twisted wires must not exceed 6.0 mm (0.25 in).