For 1990-2009 cars

#### Conversion Table of Tire Pressure (Kilopascal to PSI)

kPa | psi | kPa | psi
--- | --- | --- | ---
See Vehicle Certification Label for correct tire inflation pressure and tire load installed at the factory. Tire pressure is printed in kPa and pounds per square inch (psi). The proper tire inflation pressure at the factory means the cold tire pressure. Cold means your vehicle has been parked for at least 3 hours or driven no more than 1 mile (1.6 km). Check the tire inflation pressure when the tire is cold.
140 | 20 | 215 | 31
145 | 21 | 220 | 32
155 | 22 | 230 | 33
160 | 23 | 235 | 34
165 | 24 | 240 | 35
170 | 25 | 250 | 36
180 | 26 | 275 | 40
185 | 27 | 310 | 45
190 | 28 | 345 | 50
200 | 29 | 380 | 55
205 | 30 | 415 | 60
Conversion: 6.9 kPa=1 psi