For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accelerator Pedal Position (APP) Sensor Bolt | 9 N·m | 80 lb in
Air Cleaner Bolt | 9 N·m | 80 lb in
Air Cleaner Cover Screw | 8 N·m | 71 lb in
Air Cleaner Duct Clamps | 4 N·m | 35 lb in
Barometric Pressure Sensor Bolt | 10 N·m | 89 lb in
Camshaft Position Actuator Solenoid Valve | 10 N·m | 89 lb in
Camshaft Position (CMP) Sensor Bolt | 10 N·m | 89 lb in
Crankshaft Position (CKP) Sensor Bolt | 10 N·m | 89 lb in
Engine Coolant Temperature (ECT) Sensor | 22 N·m | 16 lb ft
Evaporative Emission (EVAP) Canister Nut | 6 N·m | 53 lb in
Fuel Filler Tube Bolt | 3.5 N·m | 31 lb in
Fuel Filler Tube Brace Bolt | 9 N·m | 80 lb in
Fuel Filler Tube Hose Clamp | 3.5 N·m | 31 lb in
Fuel Filter Bracket Bolt | 9 N·m | 80 lb in
Fuel Filter Outlet Fitting | 30 N·m | 22 lb ft
Fuel Rail Bolt | 10 N·m | 89 lb in
Fuel Tank Strap Bolt | 50 N·m | 37 lb ft
Heated Oxygen Sensors (HO2S) | 43 N·m | 32 lb ft
Ignition Coil Bolt | 10 N·m | 89 lb in
Intake Manifold Runner Control Solenoid Bolt | 10 N·m | 89 lb in
Knock Sensor Bolt | 23 N·m | 17 lb ft
MAF Sensor Screw | 4 N·m | 35 lb in
Rear Frame Bolt | 200 N·m | 148 lb ft
Shock Bolt - Lower | 90 N·m | 66 lb ft
Spark Plug | 20 N·m | 15 lb ft
Throttle Body Bolt | 10 N·m | 89 lb in