For 1990-2009 cars

### Removal Procedure

1. Remove the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement.
2. Remove the bolts securing the left side ground strap to the cam cover and the engine block.
3. Remove the left side ground strap from the engine.
4. Remove the bolts securing the right side ground strap to the cam cover and the engine block.
5. Remove the right side ground strap from the cylinder head.

### Installation Procedure

1. Install the right side ground strap into the vehicle.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the right side ground strap to the cam cover bolt and tighten to 10 N·m (89 lb in).
3. Install the right side ground strap to the cylinder head bolt and tighten to 25 N·m (18 lb ft).
4. Install the left side ground strap into the vehicle.
5. Install the left side ground strap to the cam cover bolt and tighten to 10 N·m (89 lb in).
6. Install the left side ground strap to the cylinder head bolt and tighten to 25 N·m (18 lb ft).
7. Install the fuel injection sight shield. Refer to Fuel Injector Sight Shield Replacement.