For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel compartment. Refer to Instrument Panel Compartment Replacement.
2. Remove the right insulator panel. Refer to Instrument Panel Insulator Replacement - Right Side.
3. Remove the blower and the upper air inlet assembly bolts (1).
4. Remove the lower right air inlet assembly bolt (1).
5. Slide the assembly to the right and then lower.
6. Disconnect the air inlet assembly electrical connector (1).
7. Rotate blower and the air inlet assembly (1) and remove.

### Installation Procedure

1. Connect blower and the air inlet assembly electrical connector (1).
2. Install the air inlet assembly (1) to the locator pin.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the upper air inlet assembly bolts (1).

Tighten
Tighten the bolt to 9 N·m (80 lb in).

4. Install the lower right air inlet assembly bolt (1).

Tighten
Tighten the bolt to 9 N·m (80 lb in).

5. Install the instrument panel compartment. Refer to Instrument Panel Compartment Replacement.
6. Install the insulator panel. Refer to Instrument Panel Insulator Replacement - Right Side.