For 1990-2009 cars

### Removal Procedure

1. Remove the instrument cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement .
2. Remove the bolts securing the instrument cluster.
3. Disconnect the electrical connector and remove the instrument cluster.

### Installation Procedure

1. Disconnect the electrical connector and install the instrument cluster.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolts securing the instrument cluster.

Tighten
Tighten the bolts to 2 N·m (9 lb in).

3. Install the instrument cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement .