For 1990-2009 cars

### Removal Procedure

1. Remove the engine oil pan. Refer to Oil Pan Replacement.
2. Remove the oil pump pipe support bracket nut.
3. Remove the oil pump pipe bolt.
4. Remove the oil pump pipe and screen assembly.
5. Remove and discard the oil pump pipe gasket.

### Installation Procedure

1. Install a NEW oil pump pipe gasket on the oil pump pipe.
2. Install the oil pump pipe and screen assembly.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the oil pump pipe and screen assembly retaining bolt and nut.

Tighten

• | Tighten the oil pump pick-up tube nut to 24 N·m (18 lb ft).

• | Tighten the oil pump pick-up tube bolt to 10 N·m (89 lb in).

4. Install the oil pan. Refer to Oil Pan Replacement.