For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Compressor Bolt - Front | 25 N·m | 18 lb ft
A/C Compressor Bolt - Rear | 23 N·m | 17 lb ft
A/C Compressor and Power Steering Bracket Bolt | 50 N·m | 37 lb ft
A/C Drive Belt Tensioner Bolt | 50 N·m | 37 lb ft
Block Coolant Drain Hole Plug | 20 N·m | 15 lb ft
Cable Bolt | 13 N·m | 115 lb in
Camshaft Bearing Cap Bolt | 12 N·m | 106 lb in
Camshaft Cover Bolt | 10 N·m | 89 lb in
Camshaft Cover Ground Strap | 25 N·m | 18 lb ft

- Camshaft Cover Bolt

10 N·m

89 lb in

- Cylinder Head Bolt

25 N·m

18 lb ft

Camshaft Intermediate Drive Shaft

- Bolt

15 N·m

11 lb ft

- Sprocket Bolt

60 N·m

44 lb ft

Camshaft Position Actuator Bolt | 120 N·m | 89 lb ft
Camshaft Position Actuator Housing Bolt | 10 N·m | 89 lb in
Camshaft Position Actuator Magnet Bolt | 8 N·m | 71 lb in
Camshaft Position Sensor Bolt | 10 N·m | 89 lb in
Connecting Rod Bolt

- First Pass

30 N·m

22 lb ft

- Second Pass

Back off to zero

- Third Pass

25 N·m

18 lb ft

- Final Pass

100 degrees

Crankshaft Balancer Bolt

- First Pass

50 N·m

37 lb ft

- Final Pass

150 degrees

Crankshaft Position Sensor and Knock Sensor Wiring Harness Bracket Bolt | 10 N·m | 89 lb in
Crankshaft Position Sensor Bolt | 10 N·m | 89 lb in
Cylinder Head Bolt

- M11

- First Pass - In Sequence

30 N·m

22 lb ft

- Second Pass - In Sequence

60 degrees

- Third Pass - In Sequence

60 degrees

- Final Pass - In Sequence

60 degrees, total 180 degrees

- M6

12 N·m

106 lb in

Cylinder Head Core Hole Threaded Plug | 80 N·m | 60 lb ft
Cylinder Head Oil Gallery Threaded Plug | 60 N·m | 44 lb ft
Drive Belt

- Generator Tensioner Bolt

50 N·m

37 lb ft

- Idler Bolt

50 N·m

37 lb ft

- Idler Nut

50 N·m

37 lb ft

ECT Sensor | 20 N·m | 15 lb ft
Engine Flywheel Bolt

- First Pass

30 N·m

22 lb ft

- Final Pass

50 degrees

Engine Front Cover Bolt | 15 N·m | 11 lb ft
Engine Mount Bracket Bolt | 60 N·m | 44 lb ft
Engine Mount Nut | 80 N·m | 59 lb ft
Engine Wiring Harness

- Front Clip Nut to Left Side Engine Mount Bracket Stud

35 N·m

26 lb ft

- Rear Clip Bolt to Left Side of Block

30 N·m

22 lb ft

- Bolt to Right Side of Block

35 N·m

26 lb ft

- Left Side Ground Bolt

12 N·m

106 lb in

- Right Side Ground to Intake Manifold Nut

8 N·m

71 lb in

EVAP Emission Canister Purge Valve Bolt | 10 N·m | 89 lb in
Exhaust Manifold

- Bolt

25 N·m

18 lb ft

- Nut

25 N·m

18 lb ft

- Pipe Hanger Bolt

50 N·m

37 lb ft

Exhaust Manifold Heat Shield Bolt | 10 N·m | 89 lb in
Exhaust Manifold Stud | 25 N·m | 18 lb ft
Fuel Rail Bolt | 10 N·m | 89 lb in
Generator Bolt | 50 N·m | 37 lb ft
Generator Rear Brace Bolt | 50 N·m | 37 lb ft
Generator Stud | 12 N·m | 106 lb in
Ignition Coil Assembly Bolt | 10 N·m | 89 lb in
Ignition Coil Assembly Stud | 10 N·m | 89 lb in
Intake Manifold

- Mounting Bolt

10 N·m

89 lb in

- Brake Booster Hose Fitting

2 N·m

18 lb in

Knock Sensor Bolt | 25 N·m | 18 lb ft
Lower Crankcase

- Bearing Bolt

- M10 x 1.5 First Pass - In Sequence

20 N·m

15 lb ft

- M10 x 1.5 Final Pass - In Sequence

65 degrees

- Perimeter Bolt

- M8 x 1.25 - In Sequence

30 N·m

22 lb ft

Oil Filter | 30 N·m | 22 lb ft
Oil Filter Adapter

- Oil Filter Bypass Hole Plug

30 N·m

22 lb ft

- Oil Filter Fitting

29 N·m

21 lb ft

- Mounting Bolt

25 N·m

18 lb ft

Oil Level Indicator Tube Bolt | 50 N·m | 37 lb ft
Oil Level Sensor | 20 N·m | 15 lb ft
Oil Manifold Plate Bolt | 10 N·m | 89 lb in
Oil Outlet Tube Bolt | 10 N·m | 89 lb in
Oil Pan Bolt

- First Pass

15 N·m

11 lb ft

- Final Pass

50 degrees

Oil Pan Baffle Bolt | 12 N·m | 106 lb in
Oil Pan Bolt

- First Pass

15 N·m

11 lb ft

- Final Pass

50 degrees

Oil Pan Bolt - Long

- First Pass

15 N·m

11 lb ft

- Final Pass

90 degrees

Oil Pan Drain Plug | 25 N·m | 18 lb ft
Oil Pressure Switch | 20 N·m | 15 lb ft
Oil Pump

- Cover Bolt

12 N·m

106 lb in

- Mounting Bolt

- First Pass

10 N·m

89 lb in

- Final Pass

35 degrees

Oil Suction Tube

- Bolt

10 N·m

89 lb in

- Nut

24 N·m

18 lb ft

Oxygen Sensor | 42 N·m | 31 lb ft
Plenum Duct Clamp | 2.25 N·m | 20 lb in
Power Steering Pump Bolt | 25 N·m | 18 lb ft
Power Steering Pump Bracket Bolt | 50 N·m | 37 lb ft
Power Steering Pump Reservoir Bracket Nut | 10 N·m | 89 lb in
Primary Camshaft Drive Chain

- Guide Bolt

25 N·m

18 lb ft

- Tensioner Bolt

25 N·m

18 lb ft

Radiator Hose Bracket Bolt | 10 N·m | 89 lb in
Secondary Camshaft Drive Chain

- Guide Bolt

25 N·m

18 lb ft

- Shoe Bolt

25 N·m

18 lb ft

- Tensioner Bolt

25 N·m

18 lb ft

Sight Shield

- Bracket Nut

10 N·m

89 lb in

- Retainer

7 N·m

62 lb in

Spark Plug | 15 N·m | 11 lb ft
Starter Motor Bolt | 30 N·m | 22 lb ft
Starter Motor Wiring Harness

- Generator Nut

20 N·m

15 lb ft

- Starter Nut - Large

10 N·m

89 lb in

- Starter Nut - Small

4 N·m

35 lb in

Thermostat Housing Bolt | 10 N·m | 89 lb in
Throttle Body Bolt | 10 N·m | 89 lb in
Water Outlet Housing Bolt | 25 N·m | 18 lb ft
Water Pump Bolt | 10 N·m | 89 lb in
Water Pump Pulley Bolt | 10 N·m | 89 lb in