For 1990-2009 cars

#### Special Tools

• | EN 46111 Crankshaft Rotation Socket

• | J 45059 Angle Meter

Important: Ensure that the crankshaft is in the timing drive assembly position using the EN 46111 .

1. Ensure the cylinder head locating pins are securely mounted in the cylinder block deck face.
2. Install a NEW right cylinder head gasket using the deck face locating pins for retention.
3. Align the right cylinder head with the deck face locating pins.
4. Place the right cylinder head in position on the deck face.

Notice: Refer to Fastener Notice in the Preface section.

Important: DO NOT allow oil on the cylinder head bolt bosses.

Important: DO NOT reuse the old M11 cylinder head bolts.

5. Install new M11 cylinder head bolts.

Tighten

1. Tighten the M11 cylinder head bolts a first pass in sequence to 30 N·m (22 lb ft).
2. Tighten the M11 cylinder head bolts a second pass in sequence an additional 120 degrees using the J 45059 .