For 1990-2009 cars

### Generator Drive Belt Tensioner

1. Remove the generator drive belt tensioner bolt.
2. Remove the generator drive belt tensioner.
3. Remove the generator bracket bolts.
4. Remove the generator bracket.

### Power Steering (P/S) Pump and Air Conditioning (A/C) Compressor Drive Belt Tensioner

1. Remove the P/S pump and A/C compressor drive belt tensioner bolt.
2. Remove the P/S pump and A/C compressor drive belt tensioner.