For 1990-2009 cars

#### Fastener Tightening Specifications

Application | Specification
--- | ---
Metric | English
Lower Control Arm to Knuckle Ball Stud Retaining Nut | 84 N·m | 62 lb ft
Lower Control Arm to Cradle Nuts | 135 N·m | 100 lb ft
Power Steering Gear to Cradle Mounting Bolts | 180 N·m | 133 lb ft
Shock Absorber MR Nut | 20 N·m | 15 lb ft
Shock Absorber Retaining Nut | 25 N·m | 18 lb ft
Shock Module to Body Retainer Bolts | 114 N·m | 84 lb ft
Shock Absorber Support Nut | 86 N·m | 63 lb ft
Shock Absorber Support Lower Control Arm Retaining Nut | 180 N·m | 133 lb ft
Stabilizer Shaft Bracket Bolts | 110 N·m | 81 lb ft
Stabilizer Shaft Link Upper Nuts (Connect Stabilizer Shaft) | 114 N·m | 84 lb ft
Stabilizer Shaft Link Lower Nut (Connect Lower Control Arm) | 125 N·m | 92 lb ft
Tie Rod Retaining Nut | 82 N·m | 60 lb ft
Upper Control Arm Ball Stud Retaining Nut | 84 N·m | 62 lb ft
Wheel Bearing/Hub Mounting Bolts | 135 N·m | 100 lb ft
Wheel Driveshaft Retaining Nut | 160 N·m | 118 lb ft