For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation.
3. Remove the stabilizer shaft link to stabilizer shaft retaining nut.
4. Disconnect the stabilizer shaft links from the stabilizer shaft.
5. Remove the stabilizer shaft mounting bolts and brackets.
6. Remove the stabilizer shaft insulators from the stabilizer shaft.
7. Remove the stabilizer shaft from the vehicle.

### Installation Procedure

1. Install the stabilizer shaft to the vehicle.
2. Install the stabilizer shaft insulators to the stabilizer shaft. Install the insulator to the stabilizer shaft with the slit facing rearward.

Note: Do not tighten the bolts at this time.

3. Install the stabilizer shaft brackets and mounting bolts.
4. Connect the stabilizer shaft links to the stabilizer shaft.

Caution: Refer to Fastener Caution in the Preface section.

5. Install the stabilizer shaft link retaining nut.

Tighten

• | Tighten the link upper nuts to 114 N·m (84 lb ft).

• | Tighten the bracket bolts to 110 N·m (81 lb ft).

6. Install the tire and wheel. Refer to Tire and Wheel Removal and Installation.
7. Lower the vehicle.