For 1990-2009 cars

## Tyco/AMP Connectors CM 42-Way

#### Special Tools

J-38125 Terminal Repair Kit

### Removal Procedure

1. Locate the connector position assurance (CPA) on the connector body and pull the CPA out. The CPA is on the wire harness side of connector.
2. Disconnect the connector from the component.
3. Use a small flat-bladed tool to gently pry off the dress cover by inserting the tool under the cover opposite the harness side and prying up.
4. Remove the cover.
5. Using a small flat-bladed tool, push on the side of the nose piece retainer while pushing the nose piece forward with your thumb. This will release the terminal position assurance (TPA).
6. Insert the J 38125-12A into the corresponding terminal release cavity. The release cavities are the 2 center rows of cavities on one half of the connector.
7. Pressing the J 38125-12A tool in the release cavity of the terminal you are removing, gently pull the wire out of the back of the connector. Always remember never use force when pulling a terminal out of a connector. See the release tool cross reference in the Reference Guide of the J-38125 to ensure that the correct release tool is used.

### Terminal Repair Procedure

Use the appropriate terminal and crimper in the J-38125 in order to replace the terminal.