For 1990-2009 cars

### Removal Procedure

1. Remove the fan. Refer to Fan Replacement.
2. Loosen the condenser tube from the fan shroud retainer clip ( 2 ).
3. Loosen the steering fluid tube from the fan shroud retainer clip ( 1 ).
4. Remove the cooling fan shroud retaining bolts.
5. Remove the fan and the fan shroud from the vehicle.

### Installation Procedure

1. Install the fan and the fan shroud to the vehicle.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the cooling fan shroud retaining bolts and tighten to 5.4 N·m (48 lb in).
3. Connect the condenser tube to the fan shroud retainer clip.
4. Connect the steering fluid tube to the fan shroud retainer clip.
5. Install the fan. Refer to Fan Replacement.