For 1990-2009 cars

Callout | Component Name
--- | ---

#### Front Side Door Inside Handle Cable Assembly Replacement

#### Preliminary Procedure

1. Remove the front side door trim panel, Refer to Front Side Door Trim Panel Replacement.
2. Remove the front side door water deflector. Refer to Water Deflector - Front Side Door. .

1 | Front Side Door Lock Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 5 N·m (44 lb in)
2 | Front Side Door Lock Assembly
3 | Front Side Door Lock Screw (Qty: 2) Tighten 9 N·m (80 lb in)
4 | Front Side Door Lock Assembly

#### Procedure

1. Raise the window to the full up position.
2. The following items will need to be disconnected for removal and reconnected for installation:

• | Lock cylinder rod

• | Outside handle lock rod by opening the clip

• | Lock assembly electrical connector

3. Remove the lock assembly from the door with the inside handle cable assembly attached.

5 | Front Side Door Inside Handle Cable Assembly Replacement