For 1990-2009 cars

### Removal Procedure

1. Remove the front floor console. Refer to Front Floor Console Replacement .
2. Remove the front floor console end panel. Refer to Front Floor Console Side Trim Rear Panel Replacement .
3. Remove the bolts securing the impact panel at the bottom of front floor console. Remove the impact panel.
4. Remove the bolts securing the air duct. Remove the air duct.
5. Remove the bolts securing the armrest to the bracket.
6. Remove the armrest.

### Installation Procedure

1. Install the armrest.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolts securing the armrest to the bracket.

Tighten
Tighten the bolts to 2 N·m (18 lb in).

3. Install the bolts securing the air duct.

Tighten
Tighten the bolts to 2 N·m (18 lb in).

4. Install the bolts securing the impact panel at the bottom of front floor console.

Tighten
Tighten the bolts to 2 N·m (18 lb in).

5. Install the front floor console end panel. Refer to Front Floor Console Side Trim Rear Panel Replacement .
6. Install the front floor console. Refer to Front Floor Console Replacement .