For 1990-2009 cars

#### Driver Position Module (DPM)

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
Drvr. Front Vertical Motor Command | -- | The driver position module (DPM) activates the seat front vertical motor when you select Up or Down. The motor should tilt the front of the seat in the up or down direction until it reaches the end of travel.
Drvr. Rear Vertical Motor Command | -- | The driver position module (DPM) activates the seat rear vertical motor when you select Up or Down. The motor should tilt the rear of the seat in the up or down direction until it reaches the end of its travel.
Drvr. Horizontal Motor Command | -- | The DPM activates the seat horizontal motor when you select Forward or Rearward. The motor should move the entire seat in the up or down direction until it reaches the end of its travel.
Drvr. Recline Motor Command | -- | The DPM activates the recline motor when you select Forward or Rearward. The motor should recline the seat back cushion in the forward or rearward direction until it reaches the end of travel.
Lumbar Up/Down | -- | The driver position module (DPM) activates the seat front vertical motor when you select Up or Down. The motor should move the lumbar in the up or down direction until it reaches the end of its travel.
Lumbar Forward/Backward | -- | The DPM activates the lumbar horizontal motor when you select Forward or Rearward. The motor should move the lumbar in the forward or rearward direction until it reaches the end of its travel.
Memory Exit 1 Recall | -- | The DPM activates the previously programmed seat directional motors when you select On. The motors should move the seat to the exit position for driver 1 or until you select Off.
Memory Exit 2 Recall | -- | The DPM activates the previously programmed seat directional motors when you select On. The motors should move the seat to the exit position for driver 2 or until you select Off.
Memory 1 Recall | -- | The DPM activates the previously programmed seat directional motors when you select On. The motors should move the seat to the memory position for driver 1 or until you select Off. Memory 2 Recall
Memory 2 Recall | -- | The DPM activates the previously programmed seat directional motors when you select On. The motors should move the seat to the memory position for driver 2 or until you select Off.