For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the exhaust system. Refer to Exhaust System Replacement.
3. Support the transmission with a suitable jack and a block of wood.
4. Remove the transmission support to body mounting bolts.
5. Remove the transmission to support mounting bolts.
6. Remove the transmission mount from the vehicle.

### Installation Procedure

1. Install the transmission mount to the vehicle.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the transmission to support mounting bolts.

Tighten
Tighten the bolts to 60 N·m (44 lb ft).

3. Install the transmission mount to body mounting bolts.

Tighten
Tighten the bolts to 60 N·m (44 lb ft).

4. Remove the transmission support.
5. Install the exhaust system.
6. Lower the vehicle.