For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (I/P) carrier. Refer to Instrument Panel Carrier Replacement.
2. Disconnect the mode actuator electrical connector.
3. Remove the mode actuator screws (3).
4. Remove the mode actuator.

### Installation Procedure

1. Install the mode actuator.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the mode actuator screws (2).

Tighten
Tighten the screws to 1 N·m (9 lb in).

3. Connect the electrical connector to the actuator.
4. Install the I/P carrier. Refer to Instrument Panel Carrier Replacement.