For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel compartment. Refer to Instrument Cluster Gages Inoperative .
2. Release the screws securing the Instrument Integration Module to the module bracket.
3. Disconnect the electrical connectors.

### Installation Procedure

1. Connect the electrical connectors.
2. Install the module to the bracket.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the screws that secure the module to the bracket.

Tighten
Tighten the screws to 2 N·m (18 lb in).

4. Install the instrument panel compartment. Refer to Instrument Cluster Gages Inoperative.
5. Re-program the module. Refer to Control Module References .