For 1990-2009 cars

Icon | Icon Definition
--- | ---
| Important: Twisted-pair wires provide an effective "shield" that helps protect sensitive electronic components from electrical interference. If the wires were covered with shielding, install new shielding. Refer to Splicing Twisted or Shielded Cable in Wiring Systems. In order to prevent electrical interference from degrading the performance of the connected components, you must maintain the proper specification when making any repairs to the twisted-pair wires shown :

• | The wires must be twisted a minimum of 12 turns per 31 cm (12 in) as measured anywhere along the length of the wires

• | The outside diameter of the twisted wires must not exceed 6.0 mm