For 1990-2009 cars

1. Install the engine mount bracket.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the engine mount bracket bolts.

Tighten
Tighten the engine mount bracket bolts to 60 N·m (44 lb ft).

3. Install the engine mount.
4. Install the engine mount nut.

Tighten
Tighten the engine mount nut to 80 N·m (59 lb ft).

5. Position the left knock sensor to the cylinder block as shown.
6. Install the knock sensor bolt.

Tighten
Tighten the knock sensor bolt to 23 N·m (17 lb ft).

7. Ensure proper knock sensor orientation.
8. Position a NEW exhaust manifold gasket onto the left exhaust manifold.
9. Install the exhaust manifold bolts into the left exhaust manifold.
10. Place the left exhaust manifold, exhaust manifold gasket and bolts as an assembly in position on the left cylinder head.
11. Install the exhaust manifold bolts into the left cylinder head.

Tighten
Tighten the exhaust manifold bolts to 25 N·m (18 lb ft).

12. Install the engine coolant temperature (ECT) sensor.

Tighten
Tighten the ECT sensor to 22 N·m (16 lb ft).