For 1990-2009 cars

## Rear Compartment Lid Release Switch Replacement Interior

### Removal Procedure

1. Remove the left front door trim panel. Refer to Side Door Sill Nameplate Replacement.
2. Push out the rear compartment release switch from behind the map bag under the front door trim plate.

### Installation Procedure

1. Install the rear compartment release switch to the map bag under the front door trim plate.
2. Install the left front door trim panel. Refer to Side Door Sill Nameplate Replacement.

## Rear Compartment Lid Release Switch Replacement Compartment Lid

### Removal Procedure

1. Using a flat-bladed tool, carefully remove the switch from the outside of the rear compartment lid.
2. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connectors.
2. Push the switch into the compartment sill plate and secure the retaining tab.

## Rear Compartment Lid Release Switch Replacement Exterior

Callout | Component Name
--- | ---
1 | Rear Compartment Release Switch Assembly

#### Procedure

1. Use a flat-bladed tool to remove the switch from the rear compartment lid carefully.
2. Disconnect the electrical connectors to be removed. Reconnect after the replacement.