For 1990-2009 cars

### Removal Procedure

1. Remove the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement .
2. Front windshield wiper arms. Refer to Windshield Wiper Arm Replacement .
3. Remove the air inlet grille panel (1). Refer to Air Inlet Grille Panel Replacement .
4. Disconnect the electrical connector (4) from the windshield wiper motor.
5. Remove the wiper motor module (6). Refer to Windshield Wiper System Module Replacement .
6. Remove the fasteners retaining the panel assemble to the instrument panel front end.
7. Remove the panel assembly from the vehicle.

### Installation Procedure

1. Install the air inlet housing panel assembly to the vehicle.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the fasteners retaining the panel assemble to the instrument panel front end.

Tighten
Tighten the nuts/bolt to 6 N·m (53 lb in).

3. Install the wiper motor module (6). Refer to Windshield Wiper System Module Replacement .
4. Install the electrical connector (4) to the windshield wiper motor.
5. Install the air inlet grille panel (1,3). Refer to Air Inlet Grille Panel Replacement .
6. Install the windshield wiper arms. Refer to Windshield Wiper Arm Replacement .
7. Install the injector sight shield. Refer to Fuel Injector Sight Shield Replacement .