For 1990-2009 cars

### Removal Procedure

1. Using your fingers, gently pull downward at the front edge of the overhead console.
2. Disconnect the electrical connector.
3. Remove the overhead console.

### Installation Procedure

1. Connect the electrical connector.
2. Install the overhead console into the headliner opening.
3. Ensure the locking tabs are properly positioned.
4. Press upward on the overhead console to secure the locking tabs to the console bracket.