For 1990-2009 cars

### Removal Procedure

1. Remove the right insulator panel. Refer to Instrument Panel Insulator Replacement - Right Side.
2. Remove the screws securing the instrument panel compartment.
3. Open the compartment lid and remove the screws securing the compartment.
4. Disconnect the electrical connector and remove the compartment.

### Installation Procedure

1. Connect the electrical connectors and install the compartment.
2. Install the screws securing the inside compartment.
3. Install the screws securing the compartment lower part.
4. Install the right insulator panel. Refer to Instrument Panel Insulator Replacement - Right Side.