For 1990-2009 cars

### Removal Procedure

1. Remove the air conditioning, power steering and water pump drive belt. Refer to Water Pump and Air Conditioning Compressor and Power Steering Pump Belt Replacement .
2. Loosen the drive belt tensioner bolt.
3. Remove the drive belt tensioner and bolt from the engine.

### Installation Procedure

1. Position the drive belt tensioner and bolt to the engine as an assembly.
2. Ensure that the alignment pin on the rear of the tensioner assembly is aligned with the locating hole on the engine.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the drive belt tensioner bolt.

Tighten
Tighten the drive belt tensioner bolt to 50 N·m (37 lb ft).

4. Install the air conditioning, power steering and water pump drive belt. Refer to Water Pump and Air Conditioning Compressor and Power Steering Pump Belt Replacement .