For 1990-2009 cars

### Removal Procedure

1. Remove the bridge console. Refer to Front Floor Console Extension Replacement - Center.
2. Remove the front floor console extension trim panel. Refer to Front Floor Console Extension Panel Replacement.
3. Remove the console shift lever bezel. Refer to Console Shift Lever Bezel Replacement.
4. Remove the ashtray assembly. Refer to Ashtray Side Panel Replacement.
5. Remove the bolts securing the front floor console to the I/P carrier.
6. Remove the bolts securing the rear of the front floor console to the floor.
7. Disconnect the electrical connector, and remove the front floor console rearward and upward.

### Installation Procedure

1. Connect the electrical connector, and install the front floor console.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the bolts securing the rear of front floor console to the floor.

Tighten
Tighten the bolts to 9 N·m (80 lb in).

3. Install the bolts securing the front floor console to the I/P carrier.

Tighten
Tighten the bolts to 9 N·m (80 lb in).

4. Install the ashtray assembly. Refer to Ashtray Side Panel Replacement.
5. Install the console shift lever bezel. Refer to Console Shift Lever Bezel Replacement.
6. Install the front floor console extension trim panel. Refer to Front Floor Console Extension Panel Replacement.
7. Install the bridge console. Refer to Front Floor Console Extension Replacement - Center.