For 1990-2009 cars

### Removal Procedure

1. Remove the Instrument panel (I/P) center trim. Refer to Instrument Cluster Trim Panel Replacement.
2. Remove the bolts (1) securing the radio to the I/P.
3. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolts (1) securing the radio the I/P.

Tighten
Tighten the bolts (1) to 9 N·m (80 lb in).

3. Install the I/P center trim. Refer to Instrument Cluster Trim Panel Replacement.