For 1990-2009 cars

### Circuit Description

The remote control door lock receiver (RCDLR) provides high side drive output voltage for the ignition 1 voltage circuit. The RCDLR controls the Run/Crank relay when the backup power mode is enabled.

### DTC Descriptor

The diagnostic procedure supports the following DTCs:

DTC B1370 Device Ignition 1 (ON and START) Circuit

The vehicle has DTCs including the DTC symptoms. For more information on DTC symptoms, refer to DTC Symptom Description .

DTC Symptom | DTC Symptom Descriptor
--- | ---
01 | Short to Battery
02 | A Short to Ground
04 | Open Circuit

### Conditions for Running the DTC

• | Voltage supplied to the module is in the normal operating voltage range of 9-16 volts.

• | Backup power mode is enabled.

### Conditions for Setting the DTC

• | The RCDLR detects a short to ground in the ignition 1 voltage circuit when the output is active.

• | The RCDLR detects a short to battery or an open in the ignition 1 voltage circuit when the output is inactive.

• | Any of the conditions above must be present for more than 0.375 second.

### Action Taken When the DTC Sets

The RCDLR disables the output for the current ignition cycle when a short to ground is detected.

### Conditions for Clearing the DTC

• | A current DTC clears when the malfunction is no longer present.

• | When the ignition cycle counter has reached the newly set threshold and no trouble occurs repeatedly, the history DTC will be cleared.

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Power Distribution Schematics Connector End View Reference: Master Electrical Component List
1 | Did you perform the Diagnostic System Check - Vehicle? | Go to Step 2 | Go to Diagnostic System Check - Vehicle
2 | Was the DTC symptom 04? | Go to Step 7 | Go to Step 3
3 | Was the DTC symptom 02? | Go to Step 4 | Go to Step 5
4 |

1. Turn OFF the ignition.
2. Disconnect the run/crank relay.
3. Connect a test lamp across coil cavities of the run/crank relay.
4. Turn ON the ignition, with the engine OFF.
5. Retrieve the DTCs from the remote control door lock receiver (RCDLR).

Is the code still set as current?

Go to Step 5

Go to Step 14

5 |

1. Turn OFF the ignition.
2. Connect the run/crank relay, if previously disconnected.
3. Disconnect the instrument panel module (IPM).
4. Disconnect the ignition 1 voltage circuit at the IPM connector.
5. Reconnect the IPM.
6. Turn ON the ignition, with the engine OFF.
7. Retrieve the DTCs from the RCDLR.

Is the code still set as current?

Go to Step 6

Go to Step 12

6 |

1. Turn OFF the ignition.
2. Disconnect the RCDLR.
3. Disconnect the run/crank relay.
4. Test the ignition 1 voltage circuit for a short to ground or short to voltage. Refer to Circuit Testing and Wiring Repairs .

Did you find and correct the condition?

Go to Step 15

Go to Step 10

7 |

1. Turn OFF the ignition.
2. Disconnect the run/crank relay.
3. Connect a test lamp across coil cavities of the run/crank relay.
4. Turn ON the ignition, with the engine OFF.
5. Retrieve DTCs from the RCDLR.

Is the code still set as current DTC?

Go to Step 8

Go to Step 14

8 |

1. Turn OFF the ignition.
2. Test the ground circuit of the run/crank relay for an open. Refer to Circuit Testing and Wiring Repairs .

Did you find and correct the condition?

Go to Step 15

Go to Step 9

9 |

1. Disconnect the RCDLR.
2. Test the ignition 1 voltage circuit between RCDLR and run/crank relay for an open. Refer to Circuit Testing and Wiring Repairs .

Did you find and correct the condition?

Go to Step 15

Go to Step 10

10 | Inspect for poor connections and terminal tension at the harness connector of the RCDLR module. Refer to Testing for Intermittent Conditions and Poor Connections . Did you find and correct the condition? | Go to Step 15 | Go to Step 11
11 | Replace the RCDLR module. Refer to Control Module References for replacement, setup, and programming. Did you complete the replacement? | Go to Step 15 | --
12 | Inspect for poor connections and terminal tension at the harness connector of the IPM. Refer to Testing for Intermittent Conditions and Poor Connections . Did you find and correct the condition? | Go to Step 15 | Go to Step 13
13 | Replace the IPM. Refer to Control Module References for replacement, setup, and programming. Did you complete the replacement? | Go to Step 15 | --
14 | Replace the run/crank relay. Did you complete the replacement? | Go to Step 15 | --
15 |

1. Reconnect all components.
2. Clear the DTCs with the scan tool.
3. Operate the vehicle under conditions when DTC runs as specified in supporting documents.

Does the DTC reset?

Go to Step 2

System OK